Major Tool & Machine, Inc.
Page: 1
 1458 East 19th Street
MTM N/C: 19511
Date: 03/30/06
 Indianapolis, IN 46218-4289
User ID: GRIFFITH

ENERGY INDUSTRIES OF OHIO
Customer:
Telephone:
216-496-2314
Contact:
NANCY HORTON
NKHFlowen@aol.com
E-Mail:
216-328-2001
Fax:

S005242-F/Ln:5
Customer P.O.:
SE141-116 / MODULAR COIL WINDING FORM TYPE
Part:
C5
Serial No./Qty:
8
Revision:
SE141-116
Drawing ID:

317-636-6433
Telephone:
MIKE GRIFFITH
Reported By:
Fax:
317-634-9420
E-Mail:
mGriffith@MajorTool.com

Problem:
Sheet 6, zone F2; 1.125 +/- .010 checks 1.025".
Outer portion of poloidal break between the poloidal break flanges was machined off of centerline approximately
.100".  The inner portion of the break (T section) was machined on location which caused a mismatch in the break
surface.

Proposed Disposition:
PROPOSED REPAIR
Machine the stock heavy side of the break to the correct location per the drawing.  This will blend into the area of the
T that is currently undercut.  Machine the T section to match the flange surface that was cut off of location
(approximately .100").  The slot width will finish at approximtaely 2.350" rather than 2.250".  In order to
accommodate the oversized slot, the shim thickness will need to be machined to 2.225 rather than 2.125".  The
additional .100" of stock will be added to only one surface on the shim and profile machined accordingly. (see
attachment)

  1 attachment
Number of additional pages: 

Customer Disposition:       [   ] Use As Is          [  ] Rework          [  ] Repair          [  ] Scrap          [  ] Replace

Title:
Date:

Major Tool Implemented By:

 /Open /WO:65707-5
n:\mtmapps\Mtnonc14.qrp

Major Tool and Machine, Inc.  1458 East 19th Street, Indianapolis, IN 46218-4289  Tel: 317-636-6433  Fax: 317-634-9420