Major Tool & Machine, Inc.
Page: 1
 1458 East 19th Street
MTM N/C: 19713
Date: 04/26/06
 Indianapolis, IN 46218-4289
User ID: GRIFFITH

ENERGY INDUSTRIES OF OHIO
Customer:
Telephone:
216-496-2314
Contact:
NANCY HORTON
NKHFlowen@aol.com
E-Mail:
216-328-2001
Fax:

S005242-F/Ln:5
Customer P.O.:
SE141-116 / MODULAR COIL WINDING FORM TYPE
Part:
C5
Serial No./Qty:
8
Revision:
SE141-116
Drawing ID:

317-636-6433
Telephone:
MIKE GRIFFITH
Reported By:
Fax:
317-634-9420
E-Mail:
mGriffith@MajorTool.com

Problem:
Workorder: 65707/5.0 Sub:1 Op:132
      Inspection Test #: 180  rejected: M TO MI: {g|.02|R|S|T}: -.034 TO .038  (THESE ARE PRE-GRINDING
RESULTS, SEE ATTACHMENT)
      Inspection Test #: 182  rejected: N TO NI: {g|.02|R|S|T}: -.024 TO .030  (THESE ARE PRE-GRINDING
RESULTS, SEE ATTACHMENT)
      Inspection Test #: 190  rejected: 96X
.375-16 UNC .750 DEEP
.625 C'BORE .188 DEEP: {#|.06|R|S|T}: .018 TO .075
      Inspection Test #: 200  rejected: : 2X .06-.09 X 45`: .06" TO .09 (SOME AREAS ARE ROUNDED DUE TO
GRINDING)
      Inspection Test #: 210  rejected: 8X Ø1-8 UNC THRU: {#|.01|A|B|C}: .006 TO .043
      Inspection Test #: 230  rejected: DATUM -E- FLANGE: {f|.01}: .019
      Inspection Test #: 250  rejected: DATUM -D- FLANGE: {f|.01}: .037
      Inspection Test #: 280  rejected: 8X
Ø1.13 THRU
BACK SPOT FACE Ø2.38
MIN DEPTH FOR C'UP: {#|.01|A|B|C}: .003 TO .017 / ACCEPT SPOT
      Inspection Test #: 291  rejected: 3X Ø1.885 +/- .003
Ø3.00 BACK SPOTFACE
VERIFY MIN CLEANUP: : 1.888 TO 1.892
      Inspection Test #: 311  rejected: 3X Ø1.885 +/- .003 THRU
Ø3.00 BACK SPOTFACE
VERIFY MIN CLEANUP: : 1.888 TO 1.895
      Inspection Test #: 361  rejected: Ø1.885 +/- .003 THRU
Ø3.00 BACK SPOTFACE
VERIFY MIN CLEANUP: : 1.890 / ACCEPT SPOT
      Inspection Test #: 431  rejected: 24X Ø1.885 +/- .003 THRU
Ø3.00 BACK SPOTFACE
VERIFY MIN CLEANUP: : 1.882 TO 1.8893 / ACCEPT SPOT
      Inspection Test #: 650  rejected: : 4.00 ~ .010: 3.960
      Inspection Test #: 980  rejected: : {g|.125|A|B|C}: .0208 TO .2076
      Inspection Test #: 990  rejected: DATUM -D- SIDE INNER CAST: {g|.5|A|B|C}: -.0006 TO -.3923
      Inspection Test #: 1010  rejected: DATUM -E- SIDE LARGE WING: {g|.125|A|B|C}: .020 TO .101
      Inspection Test #: 1030  rejected: DATUM -E- SIDE INNER CAST: {g|.5|A|B|C}: -.256 TO .258
      Inspection Test #: 1035  rejected: MACHINE / GRIND THIS AREA
TO PROFILE OF +.05/-.10: : -.213 TO .495

Workorder: 65707/5.0 Sub:1 Op:130
      Inspection Test #: 10  rejected: CHECK CLEARANCE OF ITEM 5 TO
ITEM 6.
: d.001 -  d.002: DIAMETRICAL GAP CHECKS UP TO .022" 

Proposed Disposition:
PROPOSE TO USE AS IS.

 /Open /WO:65707-5
n:\mtmapps\Mtnonc14.qrp

Major Tool and Machine, Inc.  1458 East 19th Street, Indianapolis, IN 46218-4289  Tel: 317-636-6433  Fax: 317-634-9420

 Major Tool & Machine, Inc.
Page: 2
 1458 East 19th Street
MTM N/C: 19713
Date: 04/26/06
 Indianapolis, IN 46218-4289
User ID: GRIFFITH

  Grinding Attachment
Number of additional pages: 

Customer Disposition:       [   ] Use As Is          [  ] Rework          [  ] Repair          [  ] Scrap          [  ] Replace

Title:
Date:

Major Tool Implemented By:

 /Open /WO:65707-5
n:\mtmapps\Mtnonc14.qrp

Major Tool and Machine, Inc.  1458 East 19th Street, Indianapolis, IN 46218-4289  Tel: 317-636-6433  Fax: 317-634-9420