Major Tool & Machine, Inc.
Page: 1
 1458 East 19th Street
MTM N/C: 21252
Date: 02/27/07
 Indianapolis, IN 46218-4289
User ID: GRIFFITH

ENERGY INDUSTRIES OF OHIO
Customer:
Telephone:
216-496-2314
Contact:
NANCY HORTON
NKHFlowen@aol.com
E-Mail:
216-328-2001
Fax:

S005242-F/Ln:5
Customer P.O.:
SE141-114 / MODULAR COIL WINDING FORM TYPE
Part:
A5
Serial No./Qty:
8
Revision:
SE141-114
Drawing ID:
W/O Links:
1-Type:W: 65709/5.0 Sub: 1 

317-636-6433
Telephone:
MIKE GRIFFITH
Reported By:
Fax:
317-634-9420
E-Mail:
mGriffith@MajorTool.com

Problem:
Workorder: 65709/5.0 Sub:1 Op:132
      Inspection Test #: 20  rejected: FLANGE PROFILE +/-.25 IN THIS AREA: : D IN TOLERANCE, E CHECKS
      UP TO +.019
      Inspection Test #: 130  rejected: OUTER AS CAST SURFACES: {g|,5|A|B|C}: -.042 / .369
      Inspection Test #: 150  rejected: 4 X .03 X 45: : .015 - .030
      Inspection Test #: 170  rejected: P TO M: {g|,2|R|T|S}: .023 / .131
      Inspection Test #: 180  rejected: DATUM D SIDE
      VERIFY SHELL INTERSECT CLEARANCE 
      USING GAGE MTMFX-3473: : REJECTED BETWEEN T HOLES: 5-9, 15-35, 40-41, 77, 88-93
      Inspection Test #: 190  rejected: M TO M1: {g|,02|R|T|S}: -.0165 / .0198
      Inspection Test #: 220  rejected: DATUM E SIDE
     VERIFY SHELL INTERSECT CLEARANCE
      USING GAGE MTMFX-3473: : REJECTED BETWEEN T HOLES: 48-51, 80-82, 87-90
      Inspection Test #: 230  rejected: N TO N1: {g|,02|R|T|S}: -.0186 / .0127
      Inspection Test #: 260  rejected: : bd.625 y .188: .621 - .624 / .17 - .196
      Inspection Test #: 280  rejected: DATUM E FLANGE: {f|,01}: .0177
      Inspection Test #: 290  rejected: DATUM D FLANGE: {f|,01}: .017
      Inspection Test #: 300  rejected: : d2.50 THRU: 2.514
      Inspection Test #: 330  rejected: 8X Ø1-8 UNC: {#|,010|A|B|C}: .046 MAX
      Inspection Test #: 350  rejected: 8X Ø1-8 UNC: {d|,010|A|B|C}: .046 MAX.
      Inspection Test #: 360  rejected: : d2.50 THRU: 2.512
      Inspection Test #: 780  rejected: INNER AS CAST SURFACES: {g|,5|A|B|C}: E=  -.289 / .068   D= -.382 / .067
      Inspection Test #: 790  rejected: WING SURFACES: {g|-,12;;;\,25|A|B|C}: E= -.206 / .005
      D= -.186 / -.172
      Inspection Test #: 795  rejected: WING POCKET SURFACES: {g|+0;;;-,25|A|C|B}: .136 / -.299
      Inspection Test #: 810  rejected: VERIFY CLEARANCE ABOVE SPOTFACE
      3" DIAMTER CYLINDER 3" HIGH
      1/4" BLEND IN RADIUS WERE
      APPLICABLE.: : HOLE #10 IN DATUM E FLANGE WILL NOT ACCEPT GAGE 

Proposed Disposition:
MTM Proposes to accept deviations as-is.

  10 page IDC attachment
Number of additional pages: 

Customer Disposition:       [   ] Use As Is          [  ] Rework          [  ] Repair          [  ] Scrap          [  ] Replace

n:\mtmapps\Mtnonc14.qrp

Major Tool and Machine, Inc.  1458 East 19th Street, Indianapolis, IN 46218-4289  Tel: 317-636-6433  Fax: 317-634-9420

 Major Tool & Machine, Inc.
Page: 2
 1458 East 19th Street
MTM N/C: 21252
Date: 02/27/07
 Indianapolis, IN 46218-4289
User ID: GRIFFITH

Title:
Date:

Major Tool Implemented By:

n:\mtmapps\Mtnonc14.qrp

Major Tool and Machine, Inc.  1458 East 19th Street, Indianapolis, IN 46218-4289  Tel: 317-636-6433  Fax: 317-634-9420