Major Tool & Machine, Inc.
Page: 1
 1458 East 19th Street
MTM N/C: 21483
Date: 03/26/07
 Indianapolis, IN 46218-4289
User ID: GRIFFITH

ENERGY INDUSTRIES OF OHIO
Customer:
Telephone:
216-496-2314
Contact:
NANCY HORTON
NKHFlowen@aol.com
E-Mail:
216-328-2001
Fax:

S005242-F/Ln:6
Customer P.O.:
 / 
Part:
A6
Serial No./Qty:
8
Revision:
SE141-114
Drawing ID:
W/O Links:
1-Type:W: 65709/6.0 Sub: 1 

317-636-6433
Telephone:
MIKE GRIFFITH
Reported By:
Fax:
317-634-9420
E-Mail:
mGriffith@MajorTool.com

Problem:
Workorder: 65709/6.0 Sub:1 Op:132
      Inspection Test #: 20  rejected: FLANGE PROFILE +/-.25 IN THIS AREA: : SEE FLANGE PROFILE
WORKSHEET
      Inspection Test #: 130  rejected: OUTER AS CAST SURFACES: {g|,5|A|B|C}: -.044 TO .346
      Inspection Test #: 170  rejected: P TO M: {g|,2|R|T|S}: .029 TO .119
      Inspection Test #: 180  rejected: DATUM D SIDE
VERIFY SHELL INTERSECT CLEARANCE
USING GAGE MTMFX-3473: : AREAS FROM T HOLES 84-94, 14-41, 5-10 REJECTED
      Inspection Test #: 190  rejected: M TO M1: {g|,02|R|T|S}: -.029 TO .018
      Inspection Test #: 220  rejected: DATUM E SIDE
VERIFY SHELL INTERSECT CLEARANCE
USING GAGE MTMFX-3473: : AREAS FROM T HOLES 84-90, 80, 47-53 REJECTED
      Inspection Test #: 230  rejected: N TO N1: {g|,02|R|T|S}: -.018 TO .021
      Inspection Test #: 260  rejected: : bd.625 y .188: DEPTH .177 - .206 & DIAMETER .617 - .619
      Inspection Test #: 270  rejected: .375-16 HOLES: {#|,06|R|T|S}: -.004 - .086
      Inspection Test #: 280  rejected: DATUM E FLANGE: {f|,01}: .0125
      Inspection Test #: 290  rejected: DATUM D FLANGE: {f|,01}: .019
      Inspection Test #: 330  rejected: 8X Ø1-8 UNC: {#|,010|A|B|C}: .011 - .077
      Inspection Test #: 340  rejected: : 8X d1-8UNC THRU: ACCEPT
      Inspection Test #: 350  rejected: 8X Ø1-8 UNC: {d|,010|A|B|C}: .011 - .077
      Inspection Test #: 390  rejected: : bd2.000-2.001 y0.990-1.000: .997-.999 / 2.0008-2.0013
      Inspection Test #: 480  rejected: Ø1.885: {#|d,06|N|A|E}: .011 - .065
      Inspection Test #: 500  rejected: Ø1.375-6 UNC: {#|d,06|N|A|E}: .011 - .065
      Inspection Test #: 530  rejected: 3X Ø1.5: {#|d,06|N|A|E}: .011 - .065
      Inspection Test #: 540  rejected: : 6X .25 - 20 UNC y .5
.030 X 45` CHAMFER: ACC/ REJ CHAMFER .05
      Inspection Test #: 780  rejected: INNER AS CAST SURFACES: {g|,5|A|B|C}: -.365 TO .17
      Inspection Test #: 795  rejected: WING POCKET SURFACES: {g|+0;;;-,25|A|C|B}: .265 TO -.48 

Proposed Disposition:
MTM PROPOSES TO ACCEPT DEVIATIONS AS IS.  DEFECTS ARE SIMILAR TO PREVIOUSLY
SUBMITTED AND ACCEPTED TYPE A CASTINGS.

  8 page attachment
Number of additional pages: 

Customer Disposition:       [   ] Use As Is          [  ] Rework          [  ] Repair          [  ] Scrap          [  ] Replace

n:\mtmapps\Mtnonc14.qrp

Major Tool and Machine, Inc.  1458 East 19th Street, Indianapolis, IN 46218-4289  Tel: 317-636-6433  Fax: 317-634-9420

 Major Tool & Machine, Inc.
Page: 2
 1458 East 19th Street
MTM N/C: 21483
Date: 03/26/07
 Indianapolis, IN 46218-4289
User ID: GRIFFITH

Title:
Date:

Major Tool Implemented By:

n:\mtmapps\Mtnonc14.qrp

Major Tool and Machine, Inc.  1458 East 19th Street, Indianapolis, IN 46218-4289  Tel: 317-636-6433  Fax: 317-634-9420