Major Tool & Machine, Inc.
Page: 1
 1458 East 19th Street
MTM N/C: 20528
Date: 09/26/06
 Indianapolis, IN 46218-4289
User ID: GRIFFITH

ENERGY INDUSTRIES OF OHIO
Customer:
Telephone:
216-496-2314
Contact:
NANCY HORTON
NKHFlowen@aol.com
E-Mail:
216-328-2001
Fax:

S005242-F/Ln:1
Customer P.O.:
 / 
Part:
B1
Serial No./Qty:
9
Revision:
SE141-115
Drawing ID:
W/O Links:
1-Type:W: 65708/1.0 Sub: 1 

317-636-6433
Telephone:
MIKE GRIFFITH
Reported By:
Fax:
317-634-9420
E-Mail:
mGriffith@MajorTool.com

Problem:
 Inspection Test #: 80  rejected: WING SURFACES: {g|-,12;;-.25|A|B|C}: -.033 TO .038
      Inspection Test #: 90  rejected: OUTER AS CAST SURFACES: {g|.5|A|C|B}: -.166 TO .275
      Inspection Test #: 140  rejected: 2X .31: : .305/.350
      Inspection Test #: 150  rejected: MACHINED SURFACES
M TO M1: {g|.02|R|S|T}: -.025 TO .022
      Inspection Test #: 160  rejected: DATUM D SIDE
VERIFY SHELL INTERSECT CLEARANCE
USING GAGE MTMFX-3473: : GAGE DOES NOT GO - T82
      Inspection Test #: 170  rejected: P TO M: {g|,2|R|S|T}: .018 TO .110
      Inspection Test #: 190  rejected: MACHINED SURFACES
N TO N1: {g|,02|R|S|T}: -.026 TO .032
      Inspection Test #: 200  rejected: DATUM E SIDE
VERIFY SHELL INTERSECT CLEARANCE
USING GAGE MTMFX-3473: : WILL NOT ACCEPT GAGE: T32-T37, T6-T11, T86-T92, T56-T49
      Inspection Test #: 210  rejected: Q TO N: {g|.2|R|S|T}: .009 TO .130
      Inspection Test #: 220  rejected: HOLE 63 THRU 73
: b.625y.188: #70-.635 #71-.647 #72-.636 #73-.633   .178/.184
      Inspection Test #: 260  rejected: : {#|,06|R|S|T}: .004 TO .078
      Inspection Test #: 340  rejected: DATUM E: {f|,01}: .019
      Inspection Test #: 350  rejected: DATUM E
: .25~ .01: .236 TO .256
      Inspection Test #: 360  rejected: DATUM D: {f|,01}: .014
      Inspection Test #: 370  rejected: DATUM D: .25~ .01: .237 TO .254
      Inspection Test #: 580  rejected: : 3x bd2.000 - 2.001
y .990 - 1.000: 1.9992 DIA. X .998 DEEP
      Inspection Test #: 870  rejected: CONFIRM THAT SCRIBE MARKS ARE
PARALLEL AND PERPENDICULAR TO
 THE WINDING AXIS.: : NOT PAR. / PERP.
      Inspection Test #: 880  rejected: 2X 1.56: : 1.76 TO 1.77
      Inspection Test #: 1000  rejected: MACHINED SURFACES: {g|,02|A|B|C}: -.026 TO .032
      Inspection Test #: 1010  rejected: AS CAST SURFACES: {g|,5|A|B|C}: -.312 TO .494
      Inspection Test #: 1020  rejected: WING SURFACES: {g|-.12;;-.25|A|B|C}: -.698 TO .115
      Inspection Test #: 1030  rejected: WING POCKET: {g|+0.0;;-.12|A|B|C}: -.173 TO .124

 /Open /WO:65708-1
n:\mtmapps\Mtnonc14.qrp

Major Tool and Machine, Inc.  1458 East 19th Street, Indianapolis, IN 46218-4289  Tel: 317-636-6433  Fax: 317-634-9420

Number of additional pages: 
   10 page IDC attachment

 Major Tool & Machine, Inc.
Page: 2
 1458 East 19th Street
MTM N/C: 20528
Date: 09/26/06
 Indianapolis, IN 46218-4289
User ID: GRIFFITH

Proposed Disposition:
PROPOSE TO ACCEPT DEVIATIONS AS IS.

Customer Disposition:       [   ] Use As Is          [  ] Rework          [  ] Repair          [  ] Scrap          [  ] Replace

Title:
Date:

Major Tool Implemented By:

 /Open /WO:65708-1
n:\mtmapps\Mtnonc14.qrp

Major Tool and Machine, Inc.  1458 East 19th Street, Indianapolis, IN 46218-4289  Tel: 317-636-6433  Fax: 317-634-9420