{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":27,"n_cols":9,"rows_kept":27,"cut":false,"hidden":false,"merged":[]}
["Loop","Colors","Series R","Cap.","Leakage","Total Length","Groups","Calculated Ideal Resistance ","Calculated Ideal Capacitance "]
["I.D.",null,"ohms","nf = 1000 pf.","MEG ohms","inches",null,"0.1149Ωper inch","0.00942nf per inch"]
["B1","Black & Brown",49,"8.8nf","4.3MΩ",370,4,{"$f":"0.1149* F3","v":42.512999999999998},{"$f":"0.00941667*F3","v":3.4841679000000001}]
["B4","Black & Red",48.49,"3.96nf","30.4MΩ",364,4,{"$f":"0.1149* F4","v":41.823599999999999},{"$f":"0.00941667*F4","v":3.42766788}]
["BB3","Black & Orange",54.2,"4.39nf","31.5MΩ",411,5,47.2239,3.8702513700000001]
["CC2","Black & Yellow",47.2,"4.15nf","13.5MΩ",365,5,41.938499999999998,3.4370845500000002]
["D6","Black & Green",46.52,"33.6nf","2.7MΩ",352,2,40.444800000000001,3.3146678400000003]
["DD3","Black & Blue",42.08,"3.7nf","∞",323,5,37.112700000000004,3.04158441]
["DD4","Black Violet",51.9,"27.4nf","2.4MΩ",410,5,47.109000000000002,3.8608347000000003]
["E3","Black & Gray",36.83,"3.1nf","∞",284,4,32.631599999999999,2.6743342800000001]
["E4","Black & White",39.6,"26.6nf","3.2MΩ",294,2,33.7806,2.7685009800000002]
["E5","Brown & Black",39.6,"24.9nf","4.0MΩ",301,2,34.584899999999998,2.8344176700000001]
["EE6","Brown & Brown",40.9,"33.6nf","2.6MΩ",270,7,31.023,2.5425009000000003]
["F5","Brown & Red",35.75,"7.6nf","4.6MΩ",320,4,36.768000000000001,3.0133344000000002]
["F9","Brown & Orange",45.25,"38.5nf","3.4MΩ",338,2,38.836199999999998,3.18283446]
["FF1","Brown & Yellow",35.92,"3.1nf","21.7MΩ",275,5,31.5975,2.5895842500000001]
["FF9","Brown & Green",38.4,"35.6nf","2.8MΩ",298,7,34.240200000000002,2.8061676600000003]
["G2","Brown & Blue",31.86,"8.95nf","4.1Ω",241,4,27.690899999999999,2.26941747]
["G8","Brown & Violet",36.19,"35.7nf","3.4MΩ",280,2,32.171999999999997,2.6366676]
["GG6","Brown & Gray","36.82Ω","32.4nf","3.0Ω",276,7,31.712400000000002,2.5990009199999999]
["H1","Brown & White","30.43Ω","7.79nf","3.9MΩ",226,4,25.967400000000001,2.12816742]
["H3","Red & Black","32.19Ω","8.5nf","3.4MΩ",242,4,27.805800000000001,2.2788341399999998]
["H11","Red & Brown","40.34Ω","21.1nf","3.6MΩ",244,2,28.035600000000002,2.2976674799999999]
["HH4","Red & Red","30.06Ω","32.8nf","3.0MΩ",300,7,34.47,2.8250009999999999]
["HH7","Red & Orange","39.7Ω","23.6nf","3.0MΩ",301,7,34.584899999999998,2.8344176700000001]
["I2","Red & Yellow","29.9Ω","35.3nf","2.5MΩ",225,2,25.852499999999999,2.1187507500000002]
["I8","Red & Green","38.71Ω","46nf","3.7MΩ",292,2,33.550800000000002,2.7496676400000002]

{"sheet":"Sheet2","index":1,"n_rows":27,"n_cols":7,"rows_kept":27,"cut":false,"hidden":false,"merged":[]}
["LOOP","Colors","Series R","Cap.","Leakage","Total Length","Groups"]
["I.D.",null,"ohms","NF = 100 PF.","MEG ohms","inches"]
["JJ4","Red & Blue","31.2Ω","30.5nf","2.8MΩ","238\"",7]
["JJ8","Red & Violet","35.85Ω","20.5nf","3.4MΩ","281\"",7]
["K6","Red & Gray","30.17Ω","59.4nf","1.8MΩ","231\"",1]
["K11","Red & White","33.7Ω","17.3nf","3.4MΩ","261\"",6]
["KK4","Orange & Black","30.35Ω","33nf","2.2MΩ","233\"",8]
["KK7","Orange & Brown","34.18Ω","6.8nf","3.8MΩ","264\"",8]
["KK8","Orange & Red","34.8Ω","24.5nf","3.8MΩ","269\"",8]
["KK10","Orange & Orange ","35.05Ω","33.6nf","2.69MΩ","312\"",7]
["L2","Orange & Yellow","33.7Ω","3.2nf","12.2MΩ","249\"",3]
["L4","Orange & Green","31.35Ω","31.3nf","2.7MΩ","242\"",1]
["L8","Orange & Blue","36.17Ω","24.6nf","3.4MΩ","267\"",1]
["LL8","Orange & Violet","35.94Ω","7.9nf","2.8MΩ","277\"",8]
["LL10","Orange & Gray","37.57Ω","3.08nf","∞","302\"",8]
["M3","Orange & White","39.14Ω","3.4nf","24.9MΩ","293\"",3]
["M7","Yellow & Black","36Ω","43.8nf","2.3MΩ","285\"",1]
["M8","Yellow & Brown","40.7Ω","43.9nf","2.5MΩ","304\"",8]
["MM6","Yellow & Red","34.3Ω","10nf","4.0MΩ","267\"",8]
["MM8","Yellow & Orange","37.43Ω","22nf","3.4MΩ","293\"",8]
["MM11","Yellow & Yellow","42.34Ω","20.2nf","2.6MΩ","328\"",8]
["N10","Yellow & Green","39.74Ω","33.3nf","2.5MΩ","305\"",1]
["O1","Yellow & Blue","43.2Ω","3.9nf","12.2MΩ","325\"",3]
["O4","Yellow & Violet","44.17Ω","4.2nf","12.7MΩ","327\"",3]
["O9","Yellow & Gray","41.6Ω","29.4nf","2.7MΩ","317\"",1]
["O11","Yellow & White","44.05Ω","34.3nf","2.8MΩ","336\"",1]
["OO2","Green & Black","36.71Ω","17.8nf","3.4MΩ","275\"",1]

{"sheet":"Sheet3","index":2,"n_rows":19,"n_cols":7,"rows_kept":19,"cut":false,"hidden":false,"merged":[]}
["Loop","Color","Searies R","nf=100pf.","Leakage","Total Length","Group"]
["I.D.",null,"ohms","nf=100pf.","Meg Ohms","Inches"]
["OO3","Green & Brown","42.9Ω","15.4nf","3.0MΩ","254\"",6]
["OO4","Green & Red","40.44Ω","3.14nf","13.5MΩ","305\"",6]
["OO7","Green & Orange","38.46Ω","36.6nf","2.8MΩ","300\"",8]
["OO10","Green & Yellow","39.3Ω","42.8nf","2.1MΩ","332\"",8]
["PP1","Green & Green","43.64Ω","25.1nf","1.8MΩ","327\"",6]
["Q2","Green& BLUE","48.85Ω","4.2nf","17.5MΩ","368\"",3]
["QQ1","Green Violet","45.77Ω","31.3nf","2.8MΩ","356\"",6]
["THO-1","Green & Gray","68.8Ω","5.7nf","12.7MΩ","518\"",5]
["THO-2","Green & White","62.5Ω","5.1nf","30.4MΩ","456\"",5]
["THO-3","Blue & Black","66.8Ω","6.2nf","7.2MΩ","497\"",5]
["THO-4","Blue & Brown","63.5Ω","10.7nf","4.3MΩ","421\"",6]
["THO-5","Blue & Red ","62.6Ω","9.9nf","3.9MΩ","470\"",6]
["TH180-1","Blue & Orange","50.03Ω","49.9nf","2.2MΩ","386\"",1]
["TH180-2","Blue & Yellow","45.5Ω","43.1nf","3.29MΩ","342\"",1]
["TH180-3","Blue & Green","44.04Ω","45nf","3.4MΩ","343\"",1]
["TH180-4","Blue & Blue","44.92Ω","41.1nf","3.3MΩ","354\"",2]
["TH180-5","Blue & Violet","51.01Ω","40.7nf","3.0MΩ","401\"",2]